17/00505/DISC - Skimmingdish Lane - consultation on discharge of conditions 2 and 6

Sun 03/12/2017 16:10

Dear Bob

**Condition 2 – external lighting** – no objection

**Condition 6 – cycle parking -**  objection

I am happy that the applicant is proposing three shelters each to accommodate 12 cycles.  The Apollo shelter type is fine.  However, there is an inconsistency in drawing TP/016.  The front elevation is of the correct size of Apollo shelter, which can accommodate 12 cycles.  However, the side elevation and the photograph are of the smaller size, which can only accommodate 10 cycles.  This error ought to be corrected, or at least annotated to make it completely clear that the 12-space shelters are to be provided and that the photo and side elevations are indicative only.

Kind regards

Joy

Joy White

Principal Transport Planner, Transport Development Control

(Cherwell and West Oxfordshire)

Oxfordshire County Council